{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["房屋建筑与装饰","安装工程"],"read":"whole","date_system":"1900"}

{"sheet":"房屋建筑与装饰","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,2],[2,3,2,4],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,5,4],[3,5,5,5],[3,6,5,6],[3,7,5,7]]}
[]
["分部分项工程量清单"]
["工程名称：电子科技大学长三角研究院食堂隔油池、排烟系统改造提升项目"]
["序号","项目名称","项目特征","计量单位","工程量","单价","合价","备注"]
[]
[]
["一","隔油池改造"]
[1,"实心砖墙","非粘土烧结实心砖 墙厚1/2砖 M7.5水泥砂浆砌筑","m3",5.4]
[2,"块料墙面","800*800瓷砖贴面，专用胶粘剂铺贴","m2",25.42]
[3,"块料墙面","300*600瓷砖贴面，专用胶粘剂铺贴","m2",24.98]
[4,"块料楼地面","600*600防滑地砖铺贴，20mm厚1：2水泥砂浆结合层","m2",14.6]
[5,"墙面一般抹灰","20mm厚1：3水泥砂浆分层抹面","m2",69]
[6,"墙面涂膜防水","聚氨酯防水涂料 厚度1.5mm 立面","m2",50]
[7,"墙面卷材防水","高分子复合丙纶防水卷材 厚度0.6mm 立面","m2",50]
[8,"回填方","陶粒混凝土","m3",42.4]
[9,"细石混凝土楼地面","10cm厚C20混凝土地面找平，内配φ10@100螺纹钢筋网，双层双向","m2",10.8]
[10,"混凝土构件拆除","原池内1500*300*400混凝土墩，清理装车，外运运距综合","m3",0.18]
[11,"沟盖板、井盖板、井圈","1200*500*40复合井盖制安","套",9]
[12,"其他构件","C25现浇现拌混凝土小型构件，含模版","m3",2]
[13,"水泥混凝土","20cm厚C25混凝土路面恢复","m2",4]
[14,"拆除路面","原20cm混凝土路面开槽拆除，清理装车、外运运距综合","m2",4]
[15,"管道包封","C15混凝土管道包封","m3",0.72]
[16,"池槽","800*600*600路面水池（基层处理，机砖砌，粉刷，防水，盖","项",1]
[17,"防火门修复","防火门密闭修复","项",1]
["二","排烟改造"]
[18,"天棚面龙骨及饰面拆除","原600*600吊顶面板拆除及恢复","m2",150]
[19,"集成吊顶","600*600铝扣板吊顶，含配套U型轻钢龙骨、吊杆、铁件等","m2",150]
[null,"合计"]

{"sheet":"安装工程","index":1,"n_rows":52,"n_cols":8,"rows_kept":52,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,2],[2,3,2,4],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,5,4],[3,5,5,5],[3,6,5,6],[3,7,5,7]]}
[]
["分部分项工程量清单"]
["工程名称：电子科技大学长三角研究院食堂隔油池、排烟系统改造提升项目"]
["序号","项目名称","项目特征","计量单位","工程量","单价","合价","备注"]
[]
[]
["一","排烟改造"]
[1,"不锈钢板通风管道","1.名称:不锈钢罩背管\n2.规格:300*800*1.0","m2",14.3]
[2,"不锈钢板通风管道","1.名称:不锈钢外管\n2.规格:600*600*1.0","m2",84]
[3,"净化工作台","1.名称:低空净化器\n2.型号:JP-DK12\n3.产品外尺寸：610*1485*685，进出风口尺寸1415-52\n4.匹配不锈钢电场，净化效率95%\n5.增加两组UV除异味灯管","台",1]
[4,"空调器","1.名称:静音风柜\n2.基座号采用HTFC-20,抽风风量20580-23500\n3.外置电机，风柜内部带隔音消音\n4.低转速800转/m，高风压700-780,声音更低，效果更佳\n5.采用耐高温SKF轴承，寿命更久\n6.电机线圈采用纯紫铜线圈\n7.链接电缆线380V/10平方\n8.风柜底部加装接油盒","台",1]
[5,"配电箱","1.名称:风机启动变频保护器\n2.型号:380V/15KW\n3.含箱内元器件","台",1]
[6,"不锈钢板管件制作","名称：不锈钢弯头/变径\n规格：300*800*1250","m2",5.5]
[7,"不锈钢板管件制作","名称：不锈钢变径\n规格：300*800-600*600","m2",3]
[8,"不锈钢板管件制作","名称：不锈钢楼顶弯头\n规格：600*600*1250","m2",3]
[9,"不锈钢板管件制作","名称：低空净化器白铁皮弯头/变径\n规格：（600*600-1415*520）*2000","m2",8]
[10,"不锈钢板管件制作","名称：不锈钢出风口弯头\n规格：600*600-1415*520","m2",4]
[11,"设备支架","名称：风柜支架\n材质：5#角钢","Kg",3.5]
[12,"柔性接口","1.名称:风柜软接","m2",2.6]
[13,"电力电缆","铜芯电力电缆敷设 YJV-0.6/1-5*10","m",98]
[14,"电力电缆头","户内干包式电力电缆头制作、安装 10mm2及以下，铜芯，三芯及以上","个",2]
[15,"打洞（孔）","1.名称:墙体打洞\n2.规格:DN80","个",2]
[16,"管道拆除","拆除旧排烟管道 600*600*400","m2",0.96]
[17,"罩背管封前板侧板","不锈钢板300*7200","m2",2.6]
["二","隔油池改造"]
[18,"其他泵","原抽水机2台及管件拆除","台",2]
[19,"镀锌钢管","DN100镀锌钢管制安，含管件、管卡制安，管道银粉漆一遍","m",150]
[20,"螺纹阀门","止回阀 DN100","个",2]
[21,"焊接法兰阀门","DN100 不锈钢闸阀（含阀门法兰）","个",2]
[22,"法兰","DN100 不锈钢法兰","副",2]
[23,"塑料管","UPVC塑料排水管 DN150","m",3]
[24,"塑料管","UPVC塑料排水管 DN110","m",92]
[25,"离心式泵","1.名称：离心泵 \n2.流量：100M3\n3.杨程：20米\n4.功率：11KW\n5.口径DN100\n6.其他：含配套控制箱及控制线缆","台",2]
[26,"轴流通风机","1.名称：排风风机 \n2.主轴转速：1450rpm\n3.风量：2880m³/h\n4.电压：380v\n5.风压：74pa\n6.噪音：65dB","台",1]
[27,"过滤网","304不锈钢过滤网，450*450*400mm，厚度0.8","个",1]
[28,"过滤网","304不锈钢过滤网，580*580*400mm，厚度0.8","个",3]
[29,"过滤池","600*600*400mm不锈钢过滤池制安","个",3]
[30,"冲洗设备","高压水枪 圆盘式（10M）含配套进水管路、龙头及配件等","套",1]
[31,"不锈钢板通风管道","1.名称:不锈钢圆形风管\n2.规格:DN150","m2",10]
[32,"配管","1.材质:PVC\n2.规格:Φ25mm\n3.配置形式:砖、混凝土结构暗配\n4.无消防要求","m",60]
[33,"配管","1.材质:PVC\n2.规格:Φ20mm\n3.配置形式:砖、混凝土结构暗配\n4.无消防要求","m",30]
[34,"凿（压）槽","塑料管DN25以内","m",1]
[35,"配线","1.配线形式:管内穿线\n2.型号:BV-4\n3.材质:铜","m",10]
[36,"电力电缆","铜芯电力电缆敷设 YJV-0.6/1-5*4","m",40]
[37,"电力电缆头","户内干包式电力电缆头制作、安装 10mm2及以下，铜芯，三芯及以上","个",2]
[38,"管道拆除","原钢管排污管拆除","m",76]
[39,"打洞（孔）","混凝土梁钻孔 钻孔直径132mm以内","个",4]
[40,"水池清洗费","工作内容：\n1.把原先损坏的水管全部接好\n2.把原来的水泵拆出来业主回收\n3.把池子里面油垢铲除\n4.再把原池清洗干净\n5.水池垃圾油污外运\n6.含一切清洗费用","项",1]
[41,"零星工程维修费","工作内容：\n1.多处风管漏油维修\n2.食堂内原有风机烟灶维修\n3.原油烟管漏油修复费用\n4.含一切零星工程维修费用","项",1]
[42,"脚手架搭拆",null,"项",1]
[43,"高层施工增加",null,"项",1]
[null,null,"合计"]